Audio

[UNDER CONSTRUCTION…]

Powering on the system:

Mixer

Computer

Speakers (via Siemens panel)

Audio output (from computer):

Audio output should be set to Dante in Audio software

NOTE: It's best to keep the system output set to “Internal Speakers” to avoid loud/annoying beeps

Sample rate should be set to 48 kHz

IMPORTANT: the system often takes 5-10 minutes to establish the connection from the computer to ALL speakers.. This issue is duets the system having more that 32 total Dante devices (the limit of a single interface).

Using the mixer:

37 main output channels are connected to the speakers by default (access via Dante ch. 1-37)

4 subwoofer output channels are connected to the speakers by default (access via Dante ch. 45-48)

The master faders for the mains and subs are the two on the righthand side of the mixer. PLEASE BE CAREFUL TO START WITH THE FADER AT -∞ AND SKOWKY RAISE THE VOLUME TO AN ACCEPTABLE LEVEL.. Typically levels between -10 and 0 are ideal.

Troubleshooting: I'm not getting any sound!

Double-check that everything is powered on

Waited for up to 10 minutes for the connections to be established

Audio Networking