OptiTrack MoCap Cameras

To power up the OptiTrack MoCap system, follow this procedure:

Navigate to the Home page on the touch panel in the back corner of the room

Login as Admin (password can be found inside of key lockbox)

Navigate to the AV page

Toggle the power controls Nr. 13 –> Manuell –> I/O & Nr. 15 –> Manuell –> I/O to the on (green) setting in the for WAK Galerien Gessneralle (Ost) section. After about 30(?) seconds, the rings on the face of the cameras should light up

When finished, be sure to turn Nr. 13 & Nr. 15 back to the off (red) setting

Logout from the system (if it has not already automatically timed out)